**Conrod Measurement:**

1. **Ovality = Biggest Diameter Measured – Smallest Diameter Measured ≤ 0.08mm**

**Liner measurement:**

1. **Shall not exceed 225.50mm**
2. **Ovality = Biggest Diameter Measured – Smallest Diameter Measured ≤ 0.10mm**